IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Without Finishes]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "C:\Users\johns\Desktop\00_設計模型和透視\Pei-Ying model(28).ifc"
Time stamp: "2025-06-03T18:24:00"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "DDS_IFC v3.0"
Originating system: "IFC file generated by Graphisoft Archicad 28.0.0 TAI FULL Windows version (IFC add-on version: 3001 TAI FULL)."
Authorization: "The authorising person"
Application: "Archicad" version "28.0.0" identifier "IFC add-on version: 3001 TAI FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "未定義" of Organization "未定義"
  Owner history of Person "未定義" of Organization "未定義" | application "Archicad" version "28.0.0" identifier "IFC add-on version: 3001 TAI FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1748946235 (2025-06-03T10:23:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: USD
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "新竹市立培英國民中學"
  IFCSITE "場地" | latitude 25° 2′ 4.392189″ | longitude 121° 37′ 54.635442″ | elevation above sea level 0.
    IFCBUILDING "建築"
      IFCBUILDINGSTOREY "" | elevation -1510.
        contains 20 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "自定義截面 650 x 800" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 600 x 600" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          12 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 650 x 800" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "A00_結構_RC(990) 150" | names: "SW - 036" | material: layers "A00_結構_RC(990) 150" ("A00_結構_RC(990)" 150.) | property sets: AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 500 x 500" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 800 x 800" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "A00_結構_RC(990) 500" | names: "SLA - 130" | material: layers "A00_結構_RC(990) 500" ("A00_結構_RC(990)" 500.) | property sets: AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
      IFCBUILDINGSTOREY "gL" | elevation 0.
        contains 11 elements
          6 x IFCSLAB | type IFCSLABTYPE "A00_結構_RC(990) 500" | names: "SLA - 130" | material: layers "A00_結構_RC(990) 500" ("A00_結構_RC(990)" 500.) | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 650 x 800" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "1F" | elevation 290.
        contains 60 elements
          12 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 1850" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          9 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 1800" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          9 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 1850" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 1800" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 2700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 1750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 2700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, Pset_BeamCommon, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 2750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 2000" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 2000" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 2700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCSTAIR | names: "樓梯-046" | parts: 3 IFCMEMBER | property sets: Pset_StairCommon, 產品描述(表達式), 樓梯描述(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 1750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 2050" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "#弱電_AP無線網路接收器 160 x 160" | object type "COLUMN" | names: "CRE - 032" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_ColumnCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "2F" | elevation 4290.
        contains 98 elements
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射), Pset_BeamCommon
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 800 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          11 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          8 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_SC 150 x 150" | object type "COLUMN" | names: "CRE - 026" | material: "A00_結構_SC" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 800" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 650" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          9 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 650" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 1500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式), Pset_BeamCommon
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), 梁購買長度(表達式), Pset_BeamCommon, AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 650 x 800" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 650" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 800 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 梁購買長度(表達式), 通用表面數據(映射), AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          1 x IFCSTAIR | names: "樓梯-046" | parts: 3 IFCMEMBER | property sets: Pset_StairCommon, 產品描述(表達式), 樓梯描述(表達式), 通用表面數據(映射), AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "3F" | elevation 8090.
        contains 73 elements
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 800" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          10 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射), Pset_BeamCommon
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 650" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCSTAIR | names: "樓梯-046" | parts: 3 IFCMEMBER | property sets: 產品描述(表達式), 樓梯描述(表達式), Pset_StairCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
      IFCBUILDINGSTOREY "4F" | elevation 11890.
        contains 122 elements
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          17 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 22 x 700" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 梁購買長度(表達式), 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 1100" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          11 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 25 x 700" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 800" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon, 梁購買長度(表達式), 通用表面數據(映射)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 1150" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "000_4FRC鋼構接合處 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          5 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          9 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 22 x 475" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 22 x 650" | object type "BEAM" | material: "A00_結構_SC" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, Pset_BeamCommon, 梁購買長度(表達式)
          12 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 25 x 650" | object type "BEAM" | material: "A00_結構_SC" | property sets: 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 22 x 600" | object type "BEAM" | material: "A00_結構_SC" | property sets: AC_Pset_RenovationAndPhasing, 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 25 x 475" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式), Pset_BeamCommon
          1 x IFCSTAIR | names: "樓梯-046" | parts: 3 IFCMEMBER | property sets: Pset_StairCommon, 產品描述(表達式), AC_Pset_RenovationAndPhasing, 樓梯描述(表達式), 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC 25 x 500" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
      IFCBUILDINGSTOREY "5F" | elevation 15690.
        contains 71 elements
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          8 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          10 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          8 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 550" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 650" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 梁購買長度(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射), Pset_BeamCommon
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), 通用表面數據(映射)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 梁購買長度(表達式), 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 450" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCSTAIR | names: "樓梯-046" | parts: 3 IFCMEMBER | property sets: Pset_StairCommon, 樓梯描述(表達式), AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 產品描述(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 750" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "A00_結構_SC D100" | object type "BEAM" | material: "A00_結構_SC" | property sets: Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射), 梁購買長度(表達式)
      IFCBUILDINGSTOREY "RFL" | elevation 19490.
        contains 61 elements
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 450 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          7 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          9 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 850" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
          8 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          4 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 300 x 300" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          6 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), Pset_BeamCommon, AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 500" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式)
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 梁購買長度(表達式), 通用表面數據(映射), AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 400 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 300 x 600" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 450 x 250" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: Pset_BeamCommon, 通用表面數據(映射), 梁購買長度(表達式), AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "A00_結構_RC(990) 400 x 400" | object type "COLUMN" | names: "CRE - 032" | material: "A00_結構_RC(990)" | property sets: Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, 通用表面數據(映射)
          1 x IFCBEAM | type IFCBEAMTYPE "A00_結構_RC(990) 2900 x 250" | object type "BEAM" | material: "A00_結構_RC(990)" | property sets: 通用表面數據(映射), AC_Pset_RenovationAndPhasing, 梁購買長度(表達式), Pset_BeamCommon
      IFCBUILDINGSTOREY "R2FL" | elevation 21840.
        contains 18 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 400 x 300" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 300 x 300" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 650 x 300" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 400 x 400" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 300 x 400" | material: "A00_結構_RC(990)" | property sets: AC_Pset_RenovationAndPhasing

Types
  IFCCOLUMNTYPE "自定義截面 650 x 800" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "A00_結構_RC(990) 600 x 600" | COLUMN | 2 occurrences
  IFCCOLUMNTYPE "A00_結構_RC(990) 650 x 800" | COLUMN | 18 occurrences
  IFCWALLTYPE "A00_結構_RC(990) 150" | 1 occurrence
  IFCCOLUMNTYPE "A00_結構_RC(990) 500 x 500" | COLUMN | 1 occurrence
  IFCCOLUMNTYPE "A00_結構_RC(990) 800 x 800" | COLUMN | 2 occurrences
  IFCSLABTYPE "A00_結構_RC(990) 500" | 7 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 1850" | BEAM | 12 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 1800" | BEAM | 9 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 1850" | BEAM | 9 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 1800" | BEAM | 6 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 2700" | BEAM | 5 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 1750" | BEAM | 5 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 2700" | BEAM | 4 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 2750" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 2000" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 2000" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 2700" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 1750" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 2050" | BEAM | 1 occurrence
  IFCCOLUMNTYPE "#弱電_AP無線網路接收器 160 x 160" | COLUMN | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 550" | BEAM | 21 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 700" | BEAM | 8 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 500" | BEAM | 34 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 550" | BEAM | 14 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 800 x 600" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 500" | BEAM | 3 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 600" | BEAM | 21 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 400" | BEAM | 21 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 700" | BEAM | 37 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 450" | BEAM | 6 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 600" | BEAM | 8 occurrences
  IFCCOLUMNTYPE "A00_結構_SC 150 x 150" | COLUMN | 8 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 450" | BEAM | 6 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 800" | BEAM | 14 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 650" | BEAM | 4 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 400" | BEAM | 34 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 650" | BEAM | 10 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 1500" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 500" | BEAM | 33 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 750" | BEAM | 5 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 750" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 750" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 400" | BEAM | 5 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 600" | BEAM | 11 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 650" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 750" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 800 x 450" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 400 x 400" | BEAM | 16 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 600 x 500" | BEAM | 4 occurrences
  IFCBEAMTYPE "A00_結構_SC 22 x 700" | BEAM | 17 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 1100" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_SC 25 x 700" | BEAM | 11 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 300 x 700" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 1150" | BEAM | 1 occurrence
  IFCBEAMTYPE "000_4FRC鋼構接合處 500 x 700" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_SC 22 x 475" | BEAM | 9 occurrences
  IFCBEAMTYPE "A00_結構_SC 22 x 650" | BEAM | 7 occurrences
  IFCBEAMTYPE "A00_結構_SC 25 x 650" | BEAM | 12 occurrences
  IFCBEAMTYPE "A00_結構_SC 22 x 600" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_SC 25 x 475" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_SC 25 x 500" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 550" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 450" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 400" | BEAM | 3 occurrences
  IFCBEAMTYPE "A00_結構_SC D100" | BEAM | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 450 x 500" | BEAM | 1 occurrence
  IFCBEAMTYPE "A00_結構_RC(990) 500 x 850" | BEAM | 1 occurrence
  IFCCOLUMNTYPE "A00_結構_RC(990) 300 x 300" | COLUMN | 6 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 650 x 600" | BEAM | 3 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 450 x 250" | BEAM | 1 occurrence
  IFCCOLUMNTYPE "A00_結構_RC(990) 400 x 400" | COLUMN | 2 occurrences
  IFCBEAMTYPE "A00_結構_RC(990) 2900 x 250" | BEAM | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 400 x 300" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 300 x 300" | 8 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 650 x 300" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 400 x 400" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "A00_結構_RC(990) 300 x 400" | 3 occurrences

Property sets
  Pset_ColumnCommon | properties | on 18 objects (18 IFCCOLUMN)
    Reference = "A00_結構_RC(990) 650 x 800" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    Reference = "A00_結構_SC 150 x 150" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    Reference = "A00_結構_RC(990) 300 x 300" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "A00_結構_RC(990) 600 x 600" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "A00_結構_RC(990) 800 x 800" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "A00_結構_RC(990) 400 x 400" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "#弱電_AP無線網路接收器 160 x 160" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    Reference = "自定義截面 650 x 800" (IFCIDENTIFIER)
    Slope = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon: 1 more content on 1 objects not shown
  AC_Pset_RenovationAndPhasing | properties | on 549 objects (461 IFCBEAM, 42 IFCCOLUMN, 18 IFCBUILDINGELEMENTPROXY, 15 IFCMEMBER)
    Renovation Status = "New" (IFCLABEL)
  通用表面數據(映射) | properties | on 363 objects (363 IFCBEAM)
    底部表面(通用) = "00_塗料_灰白" (IFCLABEL)
    頂部表面(通用) = "00_塗料_灰白" (IFCLABEL)
  通用表面數據(映射) | properties | on 59 objects (59 IFCBEAM)
    底部表面(通用) = "00_金屬_鋅" (IFCLABEL)
    頂部表面(通用) = "00_金屬_鋅" (IFCLABEL)
  通用表面數據(映射) | quantities | on 21 objects (21 IFCBEAM)
    底部表面積(通用) = 3.424999999999955 [SQUARE_METRE]
    頂部表面積(通用) = 3.424999999999955 [SQUARE_METRE]
  通用表面數據(映射) | quantities | on 19 objects (19 IFCCOLUMN)
    底部表面積(通用) = 0.5200000000000955 [SQUARE_METRE]
    頂部表面積(通用) = 0.5200000000000802 [SQUARE_METRE]
  通用表面數據(映射) | properties | on 16 objects (16 IFCBEAM)
    底部表面(通用) = "00_塗料_橘紅" (IFCLABEL)
    頂部表面(通用) = "00_塗料_灰白" (IFCLABEL)
  通用表面數據(映射) | properties | on 14 objects (14 IFCBEAM)
    底部表面(通用) = "00_塗料_橘紅" (IFCLABEL)
    頂部表面(通用) = "00_塗料_橘紅" (IFCLABEL)
  通用表面數據(映射) | quantities | on 12 objects (12 IFCBEAM)
    底部表面積(通用) = 1.885000087313695 [SQUARE_METRE]
    頂部表面積(通用) = 1.885000087313695 [SQUARE_METRE]
  通用表面數據(映射) | quantities | on 10 objects (10 IFCBEAM)
    底部表面積(通用) = 0.007500000000000569 [SQUARE_METRE]
    頂部表面積(通用) = 0.007500000000000569 [SQUARE_METRE]
  通用表面數據(映射): 352 more contents on 468 objects not shown
  Pset_BeamCommon | properties | on 16 objects (16 IFCBEAM)
    Reference = "A00_結構_RC(990) 500 x 700" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6849.999999999909 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    Reference = "A00_結構_RC(990) 650 x 400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2900.000134328863 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    Reference = "A00_結構_SC 25 x 650" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 299.9999999999545 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    Reference = "A00_結構_RC(990) 300 x 400" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3500.000000000014 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    Reference = "A00_結構_SC 22 x 475" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 288.9999999997599 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 7 objects (7 IFCBEAM)
    Reference = "A00_結構_SC 22 x 700" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9978.000000000009 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    Reference = "A00_結構_SC 22 x 700" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 12478.00000000007 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    Reference = "A00_結構_SC 22 x 650" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 288.9999936410135 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon: 305 more contents on 389 objects not shown
  梁購買長度(表達式) | quantities | on 27 objects (27 IFCBEAM)
    最大梁跨度 = 6849.999999999909 [MILLI METRE]
    梁懸出部分 = 120. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 14 objects (14 IFCBEAM)
    最大梁跨度 = 3500.000000000014 [MILLI METRE]
    梁懸出部分 = 100. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 12 objects (12 IFCBEAM)
    最大梁跨度 = 2900.000134328863 [MILLI METRE]
    梁懸出部分 = 100. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 11 objects (11 IFCBEAM)
    最大梁跨度 = 288.9999936410135 [MILLI METRE]
    梁懸出部分 = 100. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 10 objects (10 IFCBEAM)
    最大梁跨度 = 7699.999999999989 [MILLI METRE]
    梁懸出部分 = 120. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 10 objects (10 IFCBEAM)
    最大梁跨度 = 299.9999999999545 [MILLI METRE]
    梁懸出部分 = 100. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 9 objects (9 IFCBEAM)
    最大梁跨度 = 7700.000000000003 [MILLI METRE]
    梁懸出部分 = 120. [MILLI METRE]
  梁購買長度(表達式) | quantities | on 9 objects (9 IFCBEAM)
    最大梁跨度 = 288.9999999997599 [MILLI METRE]
    梁懸出部分 = 100. [MILLI METRE]
  梁購買長度(表達式): 241 more contents on 359 objects not shown
  產品描述(表達式) | properties | on 5 objects (5 IFCSTAIR)
    樓梯子單元- 數字ID = "046" (IFCLABEL)
  產品描述(表達式) | properties | on 4 objects (4 IFCMEMBER)
    樓梯子單元- 數字ID = "063" (IFCLABEL)
  產品描述(表達式) | properties | on 4 objects (4 IFCMEMBER)
    樓梯子單元- 數字ID = "124" (IFCLABEL)
  產品描述(表達式) | properties | on 4 objects (4 IFCMEMBER)
    樓梯子單元- 數字ID = "123" (IFCLABEL)
  產品描述(表達式) | properties | on 1 object (1 IFCMEMBER)
    樓梯子單元- 數字ID = "125" (IFCLABEL)
  產品描述(表達式) | properties | on 1 object (1 IFCMEMBER)
    樓梯子單元- 數字ID = "064" (IFCLABEL)
  產品描述(表達式) | properties | on 1 object (1 IFCMEMBER)
    樓梯子單元- 數字ID = "126" (IFCLABEL)
  Pset_StairCommon | properties | on 4 objects (4 IFCSTAIR)
    NumberOfRiser = 24. (IFCCOUNTMEASURE)
    NumberOfTreads = 23. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 158.3333333333333 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    NumberOfRiser = 26. (IFCCOUNTMEASURE)
    NumberOfTreads = 25. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 153.8461538461539 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  樓梯描述(表達式) | properties | on 3 objects (3 IFCSTAIR)
    2 R + G 結果公式 = "2 x 0.16 ( R ) + 0.26 ( G ) = 0.58" (IFCLABEL)
    R + G 公式 = "0.16 ( R ) + 0.26 ( G ) = 0.58" (IFCLABEL)
    R / G 結果 = 0.6089743589743605 (IFCREAL)
    R / G 結果公式 = "0.16 ( R ) / 0.26 ( G ) = 0.61" (IFCLABEL)
    樓梯寬度縮寫 = "W" (IFCLABEL)
    踏面寬度縮寫 = "G" (IFCLABEL)
    踢步面度縮寫 = "R" (IFCLABEL)
    踢步面數量縮寫 = "編號 R" (IFCLABEL)
  樓梯描述(表達式) | quantities | on 3 objects (3 IFCSTAIR)
    2 R + G 結果 = 576.6666666666661 [MILLI METRE]
    R + G 結果 = 418.3333333333328 [MILLI METRE]
  樓梯描述(表達式) | properties | on 1 object (1 IFCSTAIR)
    2 R + G 結果公式 = "2 x 0.15 ( R ) + 0.26 ( G ) = 0.57" (IFCLABEL)
    R + G 公式 = "0.15 ( R ) + 0.26 ( G ) = 0.57" (IFCLABEL)
    R / G 結果 = 0.5917159763313623 (IFCREAL)
    R / G 結果公式 = "0.15 ( R ) / 0.26 ( G ) = 0.59" (IFCLABEL)
    樓梯寬度縮寫 = "W" (IFCLABEL)
    踏面寬度縮寫 = "G" (IFCLABEL)
    踢步面度縮寫 = "R" (IFCLABEL)
    踢步面數量縮寫 = "編號 R" (IFCLABEL)
  樓梯描述(表達式) | quantities | on 1 object (1 IFCSTAIR)
    2 R + G 結果 = 567.6923076923071 [MILLI METRE]
    R + G 結果 = 413.8461538461532 [MILLI METRE]
  樓梯描述(表達式) | properties | on 1 object (1 IFCSTAIR)
    2 R + G 結果公式 = "2 x 0.16 ( R ) + 0.26 ( G ) = 0.58" (IFCLABEL)
    R + G 公式 = "0.16 ( R ) + 0.26 ( G ) = 0.58" (IFCLABEL)
    R / G 結果 = 0.6089743589743604 (IFCREAL)
    R / G 結果公式 = "0.16 ( R ) / 0.26 ( G ) = 0.61" (IFCLABEL)
    樓梯寬度縮寫 = "W" (IFCLABEL)
    踏面寬度縮寫 = "G" (IFCLABEL)
    踢步面度縮寫 = "R" (IFCLABEL)
    踢步面數量縮寫 = "編號 R" (IFCLABEL)
  樓梯描述(表達式) | quantities | on 1 object (1 IFCSTAIR)
    2 R + G 結果 = 576.6666666666659 [MILLI METRE]
    R + G 結果 = 418.3333333333327 [MILLI METRE]